For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Intermediate Steering Shaft Lower Bolt | 34 N·m | 26 lb ft
Intermediate Steering Shaft Upper Bolt | 34 N·m | 26 lb ft
Power Steering Fluid Cooling Pipe Bracket Nut | 9 N·m | 80 lb in
Power Steering Gear Inlet and Outlet Hose Bolt | 11 N·m | 98 lb in
Power Steering Pump Bolt | 22 N·m | 17 lb ft
Steering Gear Bolt | 110 N·m | 81 lb in
Steering Gear to Steering Knuckle Nut | 35 N·m | 26 lb in
Steering Linkage Tie Rod Nut | 35 N·m | 26 lb ft
Steering Wheel Bolt | 35 N·m | 26 lb ft