For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove front side door trim panel. Refer to Front Side Door Trim Replacement.

1 | Front Side Door Check Link Bolt Caution: Refer to Fastener Caution in the Preface section. Tip Place the door in the full open position. Tighten
25 N·m(18 lb ft)

2 | Front Side Door Check Link Nut

#### Procedure

Remove the water deflector.

Tighten
9 N·m(79 lb in)

3 | Front Side Door Check