For 1990-2009 cars

### Removal Procedure

1. Remove instrument panel compartment assembly. Refer to Instrument Panel Compartment Replacement.
2. Disconnect electrical connector and remove mode control cam actuator screws (2) (Qty: 3) and remove mode control cam actuator (1).

Tip
The graphic shows Air Inlet Housing without attaching parts for better clarity.

3. Remove air inlet valve and inside air valve control cam (1).

### Installation Procedure

1. Install air inlet valve and inside air valve control cam (1).

Tip
The air inlet valve and inside air valve control cam can only be fitted in one position.

Caution: Refer to Fastener Caution in the Preface section.

2. Install mode control cam actuator (1) and Install mode control cam actuator screws (2) (Qty: 3) and connect electrical connector.

Tighten
X N·m(X lb in).

3. Install instrument panel compartment assembly. Refer to Instrument Panel Compartment Replacement.