For 1990-2009 cars

### Installation Procedure

1. Open the hood.
2. Remove the 2 timing belt upper front cover bolts (2).
3. Remove the timing belt upper front cover (1).

### Removal Procedure

1. Install the timing belt upper front cover (1).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the 2 timing belt upper front cover bolts (2) and tighten to 6 N·m (53 lb in).
3. Close the hood.