For 1990-2009 cars

## Engine Oil Cooler Inlet Pipe Replacement 2.0L Diesel LLW

### Removal Procedure

1. Remove the catalytic converter heat shield. Refer to Catalytic Converter Heat Shield Replacement.
2. Drain engine oil. Refer to Engine Oil and Oil Filter Replacement.
3. Remove the 2 engine oil cooler hose heat shield nuts (1).
4. Remove the engine oil cooler hose heat shield bolt (3).
5. Remove the engine oil cooler hose heat shield (2).
6. Remove the 2 engine oil cooler inlet hose clamps (2).
7. Remove the engine oil cooler inlet hose (1).

### Installation Procedure

1. Install the engine oil cooler inlet hose (1).
2. Install the 2 engine oil cooler inlet hose clamps (2).
3. Install the engine oil cooler hose heat shield (2).

Caution: Refer to Fastener Caution in the Preface section.

4. Install the 2 engine oil cooler hose heat shield nuts (1) and tighten to 33 N·m (25 lb ft).
5. Install the engine oil cooler hose heat shield bolt (3) and tighten to 20 N·m (15 lb ft).
6. Fill engine oil. Refer to Engine Oil and Oil Filter Replacement.
7. Remove the catalytic converter heat shield. Refer to Catalytic Converter Heat Shield Replacement.

## Engine Oil Cooler Inlet Pipe Replacement 1.6L LXV

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the engine oil cooler housing. Refer to Engine Oil Cooler Replacement.

1 | Engine Oil Cooler Inlet Pipe