For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: Refer to SIR Warning in the Preface section. Warning: Following the deployment of a side impact air bag, inspect the following parts for damage. Replace these parts if necessary:

• | The seat cushion frame

• | The seat recliner, if equipped

• | The seat adjuster

• | The seat back frame

Failure to do so may cause future personal injury.

#### Preliminary Procedure

Disable the SIR system. Refer to SIR Disabling and Enabling.

1 | Inflatable Restraint Front End Sensor Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 7.5 N·m (66 lb in)
2 | Inflatable Restraint Front End Sensor Assembly

#### Procedure

1. Disconnect electrical connector.
2. Loosen the bolt and slide the sensor out of the keyhole slot.

Tip
The bolt is integral to the sensor assembly, DO NOT remove separately.