For 1990-2009 cars

#### Special Tools

• | EN-48245 Camshaft Locking Tool

• | EN-48946 Crankshaft Locking Tool

For equivalent regional tools, refer to Special Tools .

1. Rotate the fuel pump drive sprocket that the marks (1) and (2) align.
2. Install the timing belt (1) in the following order:

Note: Examine that the timing belt is tensioned during the installation.

2.1. | Crankshaft sprocket (7)

2.2. | Water pump pulley (6)

2.3. | Fuel pump drive pulley (4)

2.4. | Timing belt idler pulley (3)

2.5. | Camshaft drive sprocket (2)

2.6. | Timing belt tensioner (5)

3. Turn the hex-key (1) tab in a counterclockwise direction to tension the belt. Turn until the point aligns with the notch (2).

Caution: Refer to Fastener Caution in the Preface section.

4. Aligning with notch (2), tighten the timing belt tensioner bolt (3) to 25 N·m (19 lb ft) .
5. Remove the EN-48946 locking tool (1) and remove the bolts (2). Remove EN-48245 locking tool (4) from the lower crankcase hole (3). Install the lower crankcase closure bolt (5) and tighten to 30 N·m (23 lb ft) .
6. Turn the crankshaft in a clockwise direction 2 cycles and check the positions from the crankshaft.

Note: If the timing marks are not aligned, repeat the forward procedure and recheck the marks. Alignment of marks is critical for engine performance and emissions.

7. Check the camshaft position.

Note:

• | Examine that the bore (1) in the camshaft (2) is on top.

• | Examine the correct positions of the camshaft and the crankshaft.

8. Install a NEW vacuum pump gasket (3).

Note: Ensure that the vacuum pump surface and cylinder head surface are clear of old gasket material.

9. Install the vacuum pump (1).

Caution: Refer to Fastener Caution in the Preface section.

10. Install the 4 vacuum pump bolts (2) and tighten to 12 N·m (107 lb in) .
11. Install the wiring harness bracket (1).
12. Install the 2 wiring harness bracket nuts (2) and tighten to 20 N·m (15 lb ft) .
13. Install 4 wiring harness clips (1) to the bracket (3).
14. Install the wiring harness plug (2).