For 1990-2009 cars

#### Special Tools

• | EN-652 Flywheel Holder

• | EN-45059 Torque Angle Sensor Kit

For equivalent regional tools, refer to Special Tools.

1. Install the EN-652 holder (1), lock the flywheel (2) via the starter ring gear.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the crankshaft balancer (1) and NEW bolt (2) with screw locking compound and tighten in 3 passes using the EN-45059 sensor kit :

2.1. | First pass to 95 N·m (70 lb ft)

2.2. | Second pass to 45 degrees

2.3. | Third pass to 15 degrees