For 1990-2009 cars

## Air Conditioning (A/C) Refrigerant Pressure Sensor Replacement 2.0L Diesel LLW

#### Special Tools

GE-39400-A Halogen Leak Detector

For equivalent regional tools, refer to LINK.

#### Removal Procedure

1. Remove front bumper fascia air deflector. Refer to Front Bumper Fascia Air Deflector Replacement.
2. Remove the air conditioning refrigerant pressure sensor wire harness connector (1).
3. Remove the air conditioning refrigerant pressure sensor (1).
4. Remove and discard the O-ring (2).

#### Installation Procedure

1. Install a new O-ring. Refer to Sealing Washer Replacement.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the air conditioning refrigerant pressure sensor and tighten to XX N·m (XX lb in).
3. Install the air conditioning refrigerant pressure sensor wire harness connector.
4. Leak test the fittings using the GE-39400-A detector .
5. Install front bumper fascia air deflector. Refer to Front Bumper Fascia Air Deflector Replacement.

## Air Conditioning (A/C) Refrigerant Pressure Sensor Replacement 1.6L LXV

#### Special Tools

GE-39400-A Halogen Leak Detector

For equivalent regional tools, refer to Special Tools.

### Removal Procedure

1. Remove front bumper fascia air deflector. Refer to Front Bumper Fascia Air Deflector Replacement.
2. Remove the refrigerant pressure sensor wire harness connector.
3. Remove the refrigerant pressure sensor (1).
4. Remove and discard the O-ring (2).

### Installation Procedure

1. Install a new O-ring (2). Refer to O-Ring Replacement

Caution: Refer to Fastener Caution in the Preface section.

2. Install the refrigerant pressure sensor (1) and tighten to XX N·m (XX lb in).
3. Install the refrigerant pressure sensor wire harness connector.
4. Leak test the fittings using the GE-39400-A detector .
5. Install front bumper fascia air deflector. Refer to Front Bumper Fascia Air Deflector Replacement.