For 1990-2009 cars

## Engine Coolant Fan Resistor Replacement 2.0L Diesel LLW

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the engine coolant fan. Refer to Engine Coolant Fan Replacement.

1 | Engine Coolant Fan Bolt (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 4 N·m (36 lb in)
2 | Engine Coolant Fan Resistor

#### Procedure

1. Disconnect the wiring connector.
2. Unclip the engine fan resistor from the engine coolant fan shroud.

## Engine Coolant Fan Resistor Replacement 1.6L LXV

### Removal Procedure

1. Disconnect the negative cable from the battery. Refer to Battery Negative Cable Disconnection and Connection.
2. Disconnect the engine coolant fan resistor wiring harness plug.
3. Remove the engine coolant fan resistor bolt (2).
4. Remove the engine coolant fan resistor (1).

### Installation Procedure

1. Install the engine coolant fan resistor (1).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the engine coolant fan resistor bolt (2) and tighten to 4 N·m (36 lb in).
3. Connect the engine coolant fan resistor wiring harness plug.
4. Connect the negative cable to the battery. Refer to Battery Negative Cable Disconnection and Connection.