For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the left wheel drive shaft. Refer to LINK.

1 | Left Front Wheel Drive Shaft Oil Seal

#### Procedure

1. For seal removal use DT-7004 slide hammer with DT-586 seal remover .
2. For seal installation use DT-8092 driver handle with DT-47790 seal installer .

#### Special Tools

• | DT-47790 Seal Installer

• | DT-7004 Slide Hammer

• | DT-8092 Driver Handle

• | DT-586 Universal Seal Remover