For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement.
2. Remove the radiator grille support reinforcement. Refer to Radiator Grille Reinforcement Support Replacement.

1 | Hood Primary and Secondary Latch Retainer Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten xx N·m (xx lb ft)
2 | Hood Primary and Secondary Latch

#### Procedure

To release the hood primary and secondary latch unhook the hood primary latch release cable.