For 1990-2009 cars

### Removal Procedure

1. Remove the fuel injector fuel feed pipe. Refer to Fuel Injector Fuel Feed Pipe Replacement.
2. Disconnect the 4 fuel injector wiring harness plugs.
3. Remove the fuel leak off clips (4) from the fuel injectors.

Note: Be careful do not damage the leak off plastic connectors on the top from the injectors.

4. Remove the 4 fuel injectors. Refer to Fuel Injector Removal.

### Install Procedure

1. Install the 4 fuel injectors. Refer to Fuel Injector Installation.
2. Install the fuel leak off clips (4) to the fuel injectors.

Note: Be careful do not damage the leak off plastic connectors on the top from the injectors.

3. Connect the 4 fuel injector wiring harness plugs.
4. Install the Fuel Injector Fuel Feed Pipe. Refer to Fuel Injector Fuel Feed Pipe Replacement.