For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Open and support the rear compartment lid.
2. Remove the body side trim panel replacement in order to expose the tail lamp pocket nuts. Refer to Body Side Trim Panel Replacement - Left Side.

1 | Tail Lamp Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb ft)
2 | Tail Lamp Control Module with Bulb Assembly Tip Rotate the control module with bulbs counter clockwise and remove from the tail lamp housing.
3 | Tail Lamp Assembly Warning: Refer to Halogen Bulb Warning in the Preface section.

#### Procedure

1. Using a blunt tool, tap gently on the tail lamp studs before attempting to remove the tail lamp assembly from the lamp pocket.
2. Pull the tail lamp assembly rearward.
3. Disconnect the tail lamp control module with bulbs assembly electrical connector.