For 1990-2009 cars

### Repair Procedure

1. Pressure test the cooling system. Refer to Cooling System Leak Testing.

Note: If the radiator is leaky, replace it. Refer to Radiator Replacement.

2. Grind the fracture surface (1) with a proper tool.
3. Drill a persistent hole in center of the fracture surface, using a 6 mm (0.24 in) drill.
4. Install the new radiator mounting pin (2).

• | Install the nut (3)

• | Install the radiator mounting pin (2) with the bolt (1)

| Note: The bolt should not be longer than 35 mm (1.38in).

Caution: Refer to Fastener Caution in the Preface section.

5. Tighten the bolt xx N·m (xx lb in).