For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the control solenoid valve and transmission control module assembly. Refer to Control Solenoid Valve and Transmission Control Module Assembly Replacement.
2. Perform the service fast learn adapt procedure. Refer to Service Fast Learn Adapts.

1 | Output Speed Sensor Bolt M6 x 18 Caution: Refer to Fastener Caution in the Preface section. Tighten 12 N·m (107 lb in)
2 | Output Speed Sensor