For 1990-2009 cars

### Removal Procedure

1. Remove the oil pan. Refer to Oil Pan Replacement.
2. Remove the oil pump suction pipe bolt (3).
3. Remove the oil pump suction pipe bolt (2).

Note: Guarantee that no dirt contaminate the oil pump suction pipe.

4. Remove the oil pump suction pipe (1).

### Installation Procedure

Note: Guarantee that no dirt contaminate the oil pump suction pipe.

1. Install the oil pump suction pipe (1).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the oil pump suction pipe bolt (2) and tighten to 11 N·m (98 lb in).
3. Install the oil pump suction pipe bolt (3) and tighten to 35 N·m (26 lb ft).
4. Install the oil pan. Refer to Oil Pan Replacement.