For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the steering column upper trim cover. Refer to Steering Column Upper Trim Cover Replacement.

1 | Steering Column Lower Trim Cover Bolt (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Steering Column Lower Trim Cover

#### Procedure

Turn the steering wheel until the bolts are reachable.