For 1990-2009 cars

## Power Windows Malfunction RPO AXG

### Diagnostic Instructions

• | Perform the Diagnostic System Check - Vehicle prior to using this diagnostic procedure.

• | Review Strategy Based Diagnosis for an overview of the diagnostic approach.

• | Diagnostic Procedure Instructions provides an overview of each diagnostic category.

### Diagnostic Fault Information

Circuit | Short to Ground | Open/High Resistance | Short to Voltage | Signal Performance
--- | --- | --- | --- | ---
Driver Window Motor B+ | 1 | 1 | -- | --
Passenger Window Motor B+ | 2 | 2 | -- | --
Driver Window Motor Control | 1 | 1 | 1 | --
Passenger Window Motor Control | 2 | 2 | 2 | --
Driver Window Motor Ground | -- | 1 | 1 | --
Driver Window Switch Ground | -- | 1,2 | 1,2 | --
Passenger Window Switch Ground | -- | 2 | 2 | --
Passenger Window Motor Ground | -- | 2 | 2 | --
1. Driver Window Malfunction 2. Passenger Window Malfunction

### Circuit/System Description

The window motors are supplied with B+ voltage which is used to power the motor and also used as a reference voltage within the logic circuit. When the driver window switch is pressed, a switch is closed causing the reference voltage in the appropriate circuit in the window motor to drop, the window motor responds by moving the window in the direction commanded.

### Reference Information

#### Schematic Reference

Moveable Window Schematics

#### Connector End View Reference

Component Connector End Views

#### Description and Operation

Power Windows Description and Operation

#### Electrical Information Reference

• | Circuit Testing

• | Connector Repairs

• | Testing for Intermittent Conditions and Poor Connections

• | Wiring Repairs

### Circuit/System Verification

1. Ignition ON, command the driver window UP and DOWN using the S79D window switch--driver. The driver window should perform the UP and DOWN functions.

⇒ | If the window does not perform the UP/DOWN function, refer to Driver Window Malfunction.

2. Command the EXPRESS UP and EXPRESS DOWN functions of the driver window by pressing the window switch past the first detent and releasing and pulling the window switch past the first detent and releasing. The driver window should perform the EXPRESS UP and EXPRESS DOWN function.

⇒ | If the window does not perform EXPRESS UP and EXPRESS DOWN function, refer to Express Feature Malfunction.

### Circuit/System Testing

#### Driver Window Malfunction

1. Ignition OFF, disconnect the X1 harness connector at the S79D window switch-driver.
2. Test for less than 1 ohm between the ground circuit terminal 1 and ground.

⇒ | If greater than the specified range, test the ground circuit for an open/high resistance.

3. Ignition ON, verify that a test lamp illuminates between the B+ circuit terminal 4 and ground.

⇒ | If the test lamp does not illuminate, test the B+ circuit for a short to ground or an open/high resistance.

4. Ignition OFF, connect the harness connector at the S79D window switch-driver and disconnect the harness connector at the M74D window motor-driver.
5. Test for less than 1 ohm between the ground circuit terminal 1 and ground.

⇒ | If greater than the specified range, test the ground circuit for an open/high resistance.

6. Ignition ON, verify that a test lamp illuminates between the B+ circuit terminal 2 and ground.

⇒ | If the test lamp does not illuminate, test the B+ circuit for a short to ground or an open/high resistance.

7. Connect a test lamp between the control circuit terminal 3 and B+.
8. Command the driver window UP by using the S79D window switch-driver. The test lamp should illuminate when commanding the UP state.

⇒ | If the test lamp is always OFF, test the control circuit for a short to voltage or an open/high resistance. If the circuit tests normal, test or replace the S79D window switch-driver.

⇒ | If the test lamp is always ON, test the control circuit for a short to ground. If the circuit tests normal, test or replace the S79D window switch-driver.

9. Connect a test lamp between the control circuit terminal 7 and B+.
10. Command the driver window DOWN by using the S79D window switch-driver. The test lamp should illuminate when commanding the DOWN state.

⇒ | If the test lamp is always OFF, test the control circuit for a short to voltage or an open/high resistance. If the circuit tests normal, test or replace the S79D window switch-driver.

⇒ | If the test lamp is always ON, test the control circuit for a short to ground. If the circuit tests normal, test or replace the S79D window switch-driver.

11. Connect a test lamp between the control circuit terminal 5 and B+.
12. Command the driver window EXPRESS DOWN by using the S79D window switch-driver. The test lamp should illuminate when commanding the EXPESS DOWN state.

⇒ | If the test lamp is always OFF, test the control circuit for a short to voltage or an open/high resistance. If the circuit tests normal, test or replace the S79D window switch-driver.

⇒ | If the test lamp is always ON, test the control circuit for a short to ground. If the circuit tests normal, test or replace the S79D window switch-driver.

13. If all circuits test normal, replace the M74D window motor-driver.

#### Express Feature Malfunction

1. Ignition ON, command the driver power window fully UP by lifting and holding the S79D window switch--driver for 5 seconds.
2. Command the power window fully DOWN by pressing and holding the S79D window switch--driver for 5 seconds.
3. Command the express up and express down functions of the window by pressing the window switch past the first detent and releasing and pulling the window switch past the first detent and releasing. The power window should perform the express up and express down function.

⇒ | If the function does not perform as specified, replace the M74D window motor-driver.

### Component Testing

#### Driver Window Switch

1. Ignition OFF, disconnect the harness connector at the S79D window switch-driver.
2. With the switch in the INACTIVE position, test for infinite resistance between the control terminals listed below:

• | Control terminal 2

• | Control terminal 3

• | Control terminal 5

• | Control terminals 6

• | Control terminal 7

• | Control terminal 8

⇒ | If less than the specified value, replace the S79D window switch-driver.

3. With each switch in the UP position, test for less than 2 ohms between the control terminals listed below:

• | Control terminal 5

• | Control terminals 6

⇒ | If greater than the specified range, replace the S79D window switch-driver.

4. With each switch in the DOWN position, test for less than 2 ohms between the control terminals listed below:

• | Control terminal 3

• | Control terminal 7

⇒ | If greater than the specified range, replace the S79D window switch-driver

### Repair Instructions

Perform the Diagnostic Repair Verification after completing the diagnostic procedure.

Front Side Door Window Regulator Motor Replacement

## Power Windows Malfunction AXG/AEF/AER

### Diagnostic Instructions

• | Perform the Diagnostic System Check - Vehicle prior to using this diagnostic procedure.

• | Review Strategy Based Diagnosis for an overview of the diagnostic approach.

• | Diagnostic Procedure Instructions provides an overview of each diagnostic category.

### Diagnostic Fault Information

Circuit | Short to Ground | Open/High Resistance | Short to Voltage | Signal Performance
--- | --- | --- | --- | ---
Driver Window Switch B+ | 1 | 1 | -- | --
Left Front Window Motor B+ | 1 | 1 | -- | B3205 B4
Passenger Window Switch B+ | 1 | 1 | -- | --
Right Front Window Motor B+ | 1 | 1 | -- | B3210 4B
Left Rear Window Motor B+ | 2 | 2 | -- | B3215 4B
Left Rear Window Switch B+ | 2 | 2 | -- | --
Right Rear Window Motor B+ | 2 | 2 | -- | B3220 4B
Right Rear Window Switch B+ | 2 | 2 | -- | --
Left Front Window Motor Control | 1 | 1 | 1 | --
Left Rear Window Motor Control | 2 | 2 | 2 | --
Right Front Window Motor Control | 1 | 1 | 1 | --
Right Rear Window Motor Control | 2 | 2 | 2 | --
Left Front Window Motor Ground | -- | 1 | 1 | B3205 B4
Left Rear Window Motor Ground | -- | 2 | 2 | B3215 4B
Right Front Window Motor Ground | -- | 1 | 1 | B3210 4B
Right Rear Window Motor Ground | -- | 2 | 2 | B3220 4B
Driver Window Switch Ground | -- | 1 | 1 | --
Left Rear Window Switch Ground | -- | 2 | 2 | --
Passenger Window Switch Ground | -- | 1 | 1 | --
Right Rear Window Switch Ground | -- | 2 | 2 | --
1. Front Window Malfunction 2. Rear Window Malfunction

### Circuit/System Description

When the left rear, right rear or right front window switch is pressed on the driver window switch, a serial data message is sent to the body control module (BCM). The BCM examines the request and checks for messages from other power window motors prohibiting the window movement. If no prohibitive messages have been received, the BCM will send a serial data message to the appropriate passenger or rear window motor which will perform the command as requested.

Each power window motor is controlled by their respective window switches. When a power window switch is activated to a desired position, power window switch will send a signal to its respective door window motor to move the window to the desired position.

### Reference Information

#### Schematic Reference

Moveable Window Schematics

#### Connector End View Reference

Component Connector End Views

#### Description and Operation

Power Windows Description and Operation

#### Electrical Information Reference

• | Circuit Testing

• | Connector Repairs

• | Testing for Intermittent Conditions and Poor Connections

• | Wiring Repairs

#### Scan Tool Reference

Control Module References for scan tool information

### Circuit/System Verification

1. Ignition ON, command Driver Window Motor Mode, Passenger Window Motor Mode, Left Rear Window Motor Mode and Right Rear Window Motor Mode with a scan tool. Each window should go Up, Down, Express Up and Express Down when changing between the commanded states.

⇒ | If a window does not perform as specified, refer to Window Motor Malfunction.

2. Command the M74D window motor-driver UP and DOWN by using the S79D window switch-driver. The M74D window motor-driver should perform the UP and DOWN commands

⇒ | If the M74D window motor-driver does perform the UP and DOWN commands, refer to Driver Window Switch Malfunction.

3. Command the M74P window motor-passenger, M74RR window motor-right rear and M74LR window motor-left rear UP and DOWN by using the S79P window switch-passenger, S79RR window switch-right rear, and S79LR window switch-left rear. Each M74 window motor should perform the UP and DOWN function from each S79 window switch.

⇒ | If the front or rear passenger window is malfunctioning, refer to Passenger/Rear Window Switch Malfunction.

4. Observe the scan tool Window Lockout Switch Indicator Command parameter while pressing and depressing the window lockout switch on the S79D window switch-driver. The parameter should change between Active and Inactive.

⇒ | If the value does not change between commanded states, replace the S79D window switch-driver.

5. Command each window to EXPRESS UP and EXPRESS DOWN by using each S79 window switch. Each window should perform the EXPRESS UP and EXPRESS DOWN functions from each switch.

⇒ | If a window does not perform EXPRESS UP and EXPRESS DOWN function, refer to Express Feature Malfunction

### Circuit/System Testing

#### Window Motor Malfunction

1. Ignition OFF, disconnect the harness connector at the appropriate M74 window motor.
2. Test for less than 1 Ω between the ground circuit terminal 1 and ground.

⇒ | If greater than the specified range, test the ground circuit for an open/high resistance.

3. Ignition ON, verify that a test lamp illuminates between the B+ circuit terminal 2 and ground.

⇒ | If the test lamp does not illuminate, test the B+ circuit for a short to ground or an open/high resistance.

4. Ignition ON, connect the harness connector at the M74 window motor. Observe the scan tool Window Motor Mode parameter while using the appropriate window switch, the parameter should change to Up, Down and Express.

⇒ | If the value does not change, replace the M74 window motor.

#### Driver Power Window Malfunction

1. Ignition OFF, connect the X1 harness connector at the S79D window switch-driver.
2. Test for less than 1 Ω between the ground circuit terminal 1 and ground.

⇒ | If greater than the specified range, test the ground circuit for and open/high resistance.

3. Ignition ON, verify that a test lamp illuminates between the B+ circuit terminal 4 and ground.

⇒ | If greater than the specified range, test the ground circuit for and open/high resistance.

4. Ignition OFF, connect the X1 harness connector at the S79D window switch-driver.
5. Ignition ON, observe the scan tool Driver Left Front Window Switch, Driver Express Master Switch, Driver Up Master Switch, Front Passenger Down Master Switch, Front Passenger Express Master Switch, Front Passenger Up Master Switch, Left Rear Down Master Switch, Left Rear Express Master Switch, Left Rear Up Master Switch, Right Rear Down Master Switch, Right Rear Express Master Switch and Right Rear Up Master Switch parameters while using the left front window switch, left rear window switch, right rear window switch and right front window switch on the S79D window switch-driver. The parameters should change from Inactive to Active.

⇒ | If all values do not change from Inactive, replace the S79D window switch-driver.

⇒ | If some values do not change, replace the S79D window switch-driver

6. Ignition OFF, disconnect the harness connector at the M74D window motor-driver.
7. Connect a test lamp between the signal circuit terminal 5 and ground.
8. Ignition ON, command the M74D window motor-driver to EXPRESS DOWN by using the S79D window switch-driver. The test lamp should illuminate during the EXPRESS DOWN command.

⇒ | If the test lamp is always OFF, test the signal circuit for a short to ground or an open/high resistance. If the circuit tests normal, test or replace the S79D window switch-driver.

⇒ | If the test lamp is always ON, test the signal circuit for a short to voltage. If the circuit tests normal, test or replace the S79D window switch-driver.

9. Connect a test lamp between the signal circuit terminal 7 and ground.
10. Command the M74D window motor-driver DOWN by using the S79D window switch-driver. The test lamp should illuminate during the DOWN command.

⇒ | If the test lamp is always OFF, test the signal circuit for a short to ground or an open/high resistance. If the circuit tests normal, test or replace the S79D window switch-driver.

⇒ | If the test lamp is always ON, test the signal circuit for a short to voltage. If the circuit tests normal, test or replace the S79D window switch-driver.

11. Connect a test lamp between the signal circuit terminal 3 and ground.
12. Command the M74D window motor-driver UP by using the S79D window switch-driver. The test lamp should illuminate during the UP command.

⇒ | If the test lamp is always OFF, test the signal circuit for a short to ground or an open/high resistance. If the circuit tests normal, test or replace the S79D window switch-driver.

⇒ | If the test lamp is always ON, test the signal circuit for a short to voltage. If the circuit tests normal, test or replace the S79D window switch-driver.

13. If all circuits test normal, replace the M74D window motor-driver.

#### Passenger/Rear Window Switch Malfunction

1. Ignition OFF, disconnect the harness connector at the appropriate S79 window switch.
2. Test for less than 1 Ω between the ground circuit terminal 1 and ground.

⇒ | If greater than the specified range, test the ground circuit for and open/high resistance.

3. Ignition ON, verify that a test lamp illuminates between the B+ circuit terminal 2 and ground

⇒ | If the test lamp does not illuminate, test the B+ circuit for a short to ground or and open/high resistance.

4. Ignition OFF, connect the harness connector at the S79 window switch.
5. Ignition ON, observe the appropriate scan tool Window Switch at Door parameter while using the S79 window switch. The parameter should change between Up and Down.

⇒ | If the values do not change, replace the S79 window switch.

6. Ignition OFF, disconnect the harness connector at the appropriate M74 window motor.
7. Test for less than 5 Ω between the ground circuit terminal 1 and ground.

⇒ | If greater than the specified range, test the ground circuit for and open/high resistance.

8. Ignition ON, verify that a test lamp illuminates between the B+ circuit terminal 2 and ground.

⇒ | If the test lamp does not illuminate, test the B+ circuit for a short to ground or an open/high resistance.

9. Connect a test lamp between the control circuit terminal 7 and ground.
10. Command the window DOWN by using the S79 window switch, the test lamp should illuminate during the DOWN command.

⇒ | If the test lamp is always OFF, test the control circuit for a short to ground or an open/high resistance. If the circuit tests normal, replace the S79 window switch.

⇒ | If the test lamp is always ON, test the control circuit for a short to voltage. If the circuit tests normal, replace the S79 window switch.

11. Connect a test lamp between the control circuit terminal 3 and ground.
12. Command the window UP by using the S79 window switch, the test lamp should illuminate during the UP command.

⇒ | If the test lamp is always OFF, test the control circuit for a short to ground or an open/high resistance. If the circuit tests normal, replace the S79 window switch.

⇒ | If the test lamp is always ON, test the control circuit for a short to voltage. If the circuit tests normal, replace the S79 window switch.

13. Connect a test lamp between the control circuit terminal 5 and ground.
14. Command to EXPRESS DOWN by using the S79 window switch, the test lamp should illuminate during the EXPRESS DOWN command.

⇒ | If the test lamp is always OFF, test the control circuit for a short to ground or an open/high resistance. If the circuit tests normal, replace the S79 window switch.

15. If the test lamp is always ON, test the control circuit for a short to voltage. If the circuit tests normal, replace the S79 window switch
16. If all circuits test normal, replace the M74 window motor.

#### Express Feature Malfunction

1. Ignition ON, command the appropriate power window fully UP by lifting and holding the appropriate S79 window switch for 5 seconds.
2. Command the power window fully DOWN by pressing and holding the S79 window switch for 5 seconds.
3. Command the express up and express down functions of the window by pressing the S79 window switch past the first detent and releasing and pulling the S79 window switch past the first detent and releasing. The power window should perform the express up and express down function.

⇒ | If the function does not perform as specified, replace the M74 window motor.

### Component Testing

#### Rear Window Switch

1. Ignition OFF, disconnect the harness connector at the appropriate rear S79 window switch.
2. Test for infinite resistance between the control terminals 6, 7 and 8 and the ground terminal 1 with the switch in the INACTIVE position.

⇒ | If less than the specified value, replace the rear S79 window switch.

3. Test for less than 2 Ω between the control terminal 6 and the ground terminal 1 with the switch in the UP position.

⇒ | If greater than the specified range, replace the rear S79 window switch.

4. Test for less than 2 Ω between the control terminal 7 and the ground terminal 1 with the switch in the DOWN position.

⇒ | If greater than the specified range, replace the rear S79 window switch

### Repair Instructions

Perform the Diagnostic Repair Verification after completing the diagnostic procedure.

• | Rear Side Door Window Switch Replacement

• | Front Side Door Window Regulator Motor Replacement

• | Rear Side Door Window Regulator Motor Replacement

## Power Windows Malfunction AEC/AED/AEQ

### Diagnostic Instructions

• | Perform the Diagnostic System Check - Vehicle prior to using this diagnostic procedure.

• | Review Strategy Based Diagnosis for an overview of the diagnostic approach.

• | Diagnostic Procedure Instructions provides an overview of each diagnostic category.

### Diagnostic Fault Information

Circuit | Short to Ground | Open/High Resistance | Short to Voltage | Signal Performance
--- | --- | --- | --- | ---
Driver Window Switch B+ | 1 | 1 | -- | --
Passenger Window Switch B+ | 2 | 2 | -- | --
Left Rear Window Switch B+ | 3 | 3 | 3 | --
Right Rear Window Switch B+ | 3 | 3 | 3 | --
Left Front Window Motor Control | 1 | 1 | 1 | --
Left Rear Window Motor Control | 3 | 3 | 3 | --
Right Front Window Motor Control | 2 | 2 | 2 | --
Right Rear Window Motor Control | 3 | 3 | 3 | --
Driver Window Switch Ground | -- | 1 | 1 | --
Left Rear Window Switch Ground | -- | 3 | 3 | --
Passenger Window Switch Ground | -- | 2 | 2 | --
Right Rear Window Switch Ground | -- | 3 | 3 | --
1. Driver Window Malfunction 2. Passenger Window Malfunction 3. Rear Window Malfunction

### Circuit/System Description

When the ignition switch is in the RUN or ACCY position, or retained accessory power (RAP) is enabled and the driver or passenger window switch or rear window switch is pressed in the down position, voltage is applied to the appropriate window motor causing that window to open. When the driver or passenger window switch is pulled in the up position, voltage is applied to the appropriate window motor in the opposite direction causing that window to close.

### Reference Information

#### Schematic Reference

Moveable Window Schematics

#### Connector End View Reference

Component Connector End Views

#### Description and Operation

Power Windows Description and Operation

#### Electrical Information Reference

• | Circuit Testing

• | Connector Repairs

• | Testing for Intermittent Conditions and Poor Connections

• | Wiring Repairs

#### Scan Tool Reference

Control Module References for scan tool information

### Circuit/System Verification

1. Ignition ON, command the driver, passenger, left rear and right rear windows UP and DOWN by using the S79D window switch-driver, S79P window switch-passenger, S79LR window switch-left rear and S79RR window switch-right rear. Each window should perform the UP and DOWN function from each switch.

⇒ | If the driver window malfunctions, refer to Driver Window Malfunction.

⇒ | If the passenger, left rear or right rear window malfunctions, refer to Passenger/Rear Window Malfunction.

2. Observe the scan tool Driver Left Front Window Switch, Driver Express Master Switch, Driver Up Master Switch, Front Passenger Down Master Switch, Front Passenger Express Master Switch, Front Passenger Up Master Switch, Left Rear Down Master Switch, Left Rear Express Master Switch, Left Rear Up Master Switch, Right Rear Down Master Switch, Right Rear Express Master Switch and Right Rear Up Master Switch parameters while using the window switches on the driver master control. The parameters should change from Inactive to Active.

⇒ | If all values do not change from Inactive, replace the S79D window switch-driver.

⇒ | If some values do not change, replace the S79D window switch-driver.

3. Observe the scan tool Window Lockout Switch Indicator Command parameter while pressing and depressing the lockout switch on the S79D window switch, driver. The parameter should change from Inactive to Active.

⇒ | If the value does not change, replace the S79D window switch-driver.

4. Command each window to EXPRESS DOWN by pressing appropriate S79 window switch past the first detent and releasing. Each window should perform the EXPRESS DOWN function.

⇒ | If a window does not perform EXPRESS DOWN function, replace the S79 window switch.

### Circuit/System Testing

#### Driver Window Malfunction

1. Ignition OFF, disconnect the harness connector at the S79D window switch-driver.
2. Test for less than 1 Ω between the ground circuit terminal 1 and ground.

⇒ | If greater than the specified range, test the ground circuit for an open/high resistance.

3. Ignition ON, verify that a test lamp illuminates between the B+ circuit terminal 4 and ground.

⇒ | If the test lamp does not illuminate, test the B+ circuit for a short to ground or an open/high resistance.

4. Ignition OFF, connect the harness connector at the S79D window switch-driver. Disconnect the harness connector at the M74D window motor-driver.
5. Connect a test lamp between the control circuit terminal A and control circuit terminal B.
6. Ignition ON, command the M74D window motor-driver UP and DOWN by using the S79D window switch-driver. The test lamp should illuminate during the UP and DOWN commands.

⇒ | If the test lamp does not illuminate during the UP or DOWN command, test either control circuit for a short to ground or an open/high resistance. If the circuits tests normal, test or replace the S79D window switch-driver.

⇒ | If the test lamp is always ON, test either control circuit for a short to voltage. If the circuits test normal, test or replace the S79D window switch-driver.

7. If all circuits test normal, test or replace the M74D window motor-driver.

#### Passenger/Rear Window Malfunction

1. Ignition OFF, disconnect the harness connector at the appropriate S79 window switch.
2. Test for less than 1 Ω between the ground circuit terminal listed below and ground:

• | Passenger window switch terminal 1

• | Right rear window switch terminal 5

• | Left rear window switch terminal 3

• | Left rear window switch terminal 5

⇒ | If greater than the specified range, test the ground circuit for an open/high resistance.

3. Ignition ON, verify that a test lamp illuminates between the B+ circuit terminal listed below and ground:

• | Passenger window switch terminal 4

• | Right rear window switch terminal 8

• | Left rear window switch terminal 8

⇒ | If the test lamp does not illuminate, test the B+ circuit for a short to ground or an open/high resistance.

4. Ignition OFF, connect the harness connector at the S79 window switch and disconnect the harness connector at the M74 window motor.
5. Connect a test lamp between the control circuit terminal A and control circuit terminal B.
6. Ignition ON, command the M74 window motor UP and DOWN by using the S79 window switch. The test lamp should illuminate during the UP and DOWN commands.

⇒ | If the test lamp does not illuminate during the UP or DOWN command, test either control circuit for a short to ground or an open/high resistance. If the circuits tests normal, test or replace the S79 window switch.

⇒ | If the test lamp is always ON, test either control circuit for a short to voltage. If the circuits test normal, test or replace the S79 window switch.

7. If all circuits test normal, test or replace the M74 window motor.

### Component Testing

#### Window Motor

1. Ignition OFF, disconnect the harness connector at the appropriate M74 window motor.
2. Install a 25A fused jumper wire between one of the control terminals and 12V. Momentarily install a jumper wire between the other control terminal and ground. Reverse the jumper wires at least two times, the M74 window motor should perform the UP/DOWN functions.

⇒ | If it does not perform as specified, replace the M74 window motor.

### Repair Instructions

Perform the Diagnostic Repair Verification after completing the diagnostic procedure.

• | Front Side Door Window Regulator Motor Replacement

• | Rear Side Door Window Regulator Motor Replacement

• | Rear Side Door Window Switch Replacement

• | Front Side Door Window Switch Replacement - Left Side

• | Front Side Door Window Switch Replacement - Right Side