For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: When a hood hold open device is being removed or installed, provide alternate support to avoid the possibility of damage to the vehicle or personal injury.

#### Preliminary Procedure

Remove the windshield washer nozzle hose. Refer to Windshield Washer Nozzle Hose Replacement.

1 | Hood Hinge Reinforcement Nut (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 26 N·m (19 lb ft)
2 | Hood

#### Procedure

1. Transfer components as necessary.
2. Adjust hood as needed. Refer to Hood Adjustment.