For 1990-2009 cars

## Starter Replacement 2.0L Diesel LLW

### Removal Procedure

1. Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the front compartment insulator. Refer to Front Compartment Insulator Replacement.
3. Remove the positive cable nut (1) from starter motor (2).
4. Remove the positive cable (5).
5. Remove the lower starter motor bolt (4).
6. Remove the negative cable (3).
7. Remove the starter motor cable nut (1) from starter motor (2).
8. Remove the starter motor cable (3).
9. Remove the upper starter motor bolt (1).
10. Remove the starter motor (2).

### Installation Procedure

1. Install the starter motor (2).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the upper starter motor bolt (1) and tighten to 58 N·m (43 lb ft).
3. Install the starter motor cable (3).
4. Install the starter motor cable nut (1) at the starter motor (2) and tighten to 9 N·m (80 lb in).
5. Install the negative cable (3).
6. Install the lower starter motor bolt (4) and tighten to 58 N·m (43 lb ft).
7. Install the positive cable (5).
8. Install the positive cable nut (1) at starter motor (2) and tighten to 9 N·m (80 lb in).
9. Install the front compartment insulator. Refer to Front Compartment Insulator Replacement.
10. Connect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.

## Starter Replacement 1.6L LXV

Callout | Component Name
--- | ---

#### Peliminary Procedure

Disconnect the negative cable from the battery. Refer to Battery Negative Cable Disconnection and Connection.

1 | Starter Motor Negative Cable Nut Caution: Refer to Fastener Caution in the Preface section. Tighten 12.5 N·m (110 lb in)
2 | Starter Motor Negative Cable
3 | Starter Motor Positive Cable Nut Tighten 12.5 N·m (110 lb in)
4 | Starter Motor Positive Cable
5 | Starter Motor Bolt Tighten 25 N·m (18 lb ft)
6 | Starter Motor Bolt Tighten 25 N·m (18 lb ft)
7 | Starter Motor