For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove outside rearview mirror glass. Refer to Outside Rearview Mirror Glass Replacement.

1 | Outside Rearview Mirror Housing Screw (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Lower Outside Rearview Mirror Housing Screw Tighten 2.5 N·m (22 lb in)
3 | Outside Rearview Mirror Housing Tip Disconnect electrical connector.