For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Front seat adjuster replacement, if equipped. Refer to Front Seat Adjuster Replacement.
2. Driver or passenger seat replacement. Refer to Driver or Passenger Seat Replacement.

1 | Seat Cushion Outer Trim Panel Screw (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Seat Cushion Outer Trim Panel