For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement.
2. Remove the radiator grille reinforcement support. Refer to Radiator Grille Reinforcement Support Replacement.

1 | Radiator Support Bracket Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 22 N·m (17 lb ft)
2 | Radiator Support Bracket

#### Procedure

Pull the radiator forward until the bracket is reachable.