For 1990-2009 cars

#### Special Tools

EN-49733 Holding Wrench

For equivalent tools, refer to Special Tools.

Note: Consider the correct position from the crankshaft sprocket on the crankshaft, otherwise it could be damaged.

1. Install the crankshaft sprocket (1).
2. Install crankshaft sprocket bolt (2).
3. Install EN-49733 holder (2) to fix the crankshaft sprocket (1).

Caution: Refer to Fastener Caution in the Preface section.

4. Tighten the crankshaft sprocket bolt (2) to 235 N·m (174 lb ft).
5. Remove EN-49733 holder (2) to fix the crankshaft sprocket (1).