For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the power steering pump belt. Refer to Power Steering Pump Belt Replacement.
2. Place drain pans under the vehicle as needed.

1 | Power Steering Gear Inlet Hose Hollow Screw Caution: Refer to Fastener Caution in the Preface section. Tighten 21 N·m (16 lb in)
2 | Power Steering Gear Inlet Hose
3 | Power Steering Reservoir Outlet Hose
4 | Power Steering Pump Bolt (Qty: 2) Tighten 22 N·m (17 lb ft)
5 | Power Steering Pump

#### Procedure

Fill and bleed the power steering system. Refer to Power Steering System Bleeding.

Tip
Clean any excess power steering fluid from the vehicle.