For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: Any time service is being performed which requires removal of the air cleaner assembly, always cover the throttle body opening. This will prevent any foreign material from entering the engine.
1 | Air Mass Flow Sensor Clamp Caution: Refer to Fastener Caution in the Preface section. Tighten 3.5 N·m (31 lb in)
2 | Air Cleaner Outlet Front Duct Clamp Tighten 3.5 N·m (31 lb in)
3 | Air Cleaner Outlet Front Duct Bolt (Qty: 2) Tighten 5 N·m (45 lb in)
4 | Air Cleaner Outlet Front Duct