For 1990-2009 cars

1. Remove the oil filter cap (1) with oil filter cap gasket (2).
2. Remove the oil filter (3).
3. Remove the oil filter housing oil drain plug (4).
4. Remove the oil filter housing oil drain plug gasket (5).
5. Remove the oil filter housing bolt (11).
6. Remove the oil filter housing (10).
7. Remove the oil filter housing gasket (9).
8. Remove the engine oil cooler bolt (8).

Note: Consider and note the engine oil cooler position for reinstalling.

9. Remove the engine oil cooler (7).
10. Remove the engine oil cooler gasket (6).