For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Battery Hold Down Retainer Nut | 9 Nm | 80 lb in
Battery Negative Cable Nut | 9 Nm | 80 lb in
Battery Positive Cable Bolt | 9 Nm | 80 lb in
Battery Positive Cable Nut | 9 Nm | 80 lb in
Battery Tray Bolt | 15 Nm | 12 lb ft
Engine Wiring Harness Bracket Bolt (1.6L LXV) | 10 Nm | 89 lb in
Engine Wiring Harness Bracket Nut (1.6L LXV) | 9 Nm | 80 lb in
Engine Wiring Harness Ground Bolt (1.6L LXV) | 10 Nm | 89 lb ft
Generator Bolt (1.6L LXV) | 35 Nm | 26 lb ft
Generator Bolt (2.0L LLW) | 58 Nm | 43 lb ft
Generator Nut (2.0L LLW) | 58 Nm | 43 lb ft
Generator Positive Cable Nut (1.6L LXV) | 7 N·m | 62 lb in
Generator Wiring Harness Nut (1.6L LXV) | 7 N·m | 62 lb in
Ground Cable Nut | 9 Nm | 80 lb in
Knock Sensor Bolt (1.6L LXV) | 20 Nm | 15 lb ft
Starter Bolt (1.6L LXV) | 18 Nm | 14 lb ft
Starter Bolt (2.0L LLW) | 58 Nm | 43 lb ft
Starter Motor Cable Nut (2.0L LLW) | 9 Nm | 80 lb in
Starter Motor Ground Cable Nut and Stud | 12.5 N·m | 111 lb in
Starter Motor Negative Cable (1.6L LXV) | 12.5 N·m | 111 lb in
Starter Motor Positive Cable (1.6L LXV) | 12.5 N·m | 111 lb in

- (1) = Use NEW fastening nuts. (2) = Use NEW fastening bolts. (3) = Recut threads before re-use and insert bolts with screw locking compound - red. The installation time, including torque inspection, is a maximum of 10 minutes. (4) = Insert NEW fastening bolts with screw locking compound