For 1990-2009 cars

### Removal Procedure

1. Remove instrument panel lower trim panel - left side. Refer to Instrument Panel Lower Trim Panel Replacement - Left Side.
2. Remove instrument outer trim cover - left side. Refer to Instrument Panel Outer Trim Cover Replacement - Left Side.
3. Remove instrument panel lower trim pad cover - left side. Refer to Instrument Panel Lower Trim Pad Cover Replacement.
4. Remove radio cooling duct (1).

### Installation Procedure

1. Install radio cooling duct (1).
2. Install instrument panel lower trim pad cover - left side. Refer to Instrument Panel Lower Trim Pad Cover Replacement.
3. Install instrument outer trim cover - left side. Refer to Instrument Panel Outer Trim Cover Replacement - Left Side.
4. Install instrument panel lower trim panel - left side. Refer to Instrument Panel Lower Trim Panel Replacement - Left Side.