For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the rear side door sill trim plate. Refer to Rear Side Door Sill Trim Plate Replacement.
2. Remove the rear seat back. Refer to LINK.
3. Remove the quarter window garnish molding. Refer to Quarter Window Garnish Molding Replacement.

1 | Rear Window Panel Trim Retainer Clip
2 | Body Side Trim Panel Retainer (Qty: 3)
3 | Body Side Trim Panel Assembly