For 1990-2009 cars

## Water Pump Pulley Replacement 1.6L LXV

### Removal Procedure

1. Remove the air cleaner housing. Refer to Air Cleaner Assembly Replacement.
2. Loosen the 3 water pump pulley bolts (1).

Note: Counterhold against crankshaft balancer bolt.

3. Remove the drive belt. Refer to Drive Belt Replacement.
4. Remove the 3 water pump pulley bolts (1).
5. Remove the water pump pulley (2) from the water pump (3).

### Installation Procedure

1. Install the water pump pulley (2) to the water pump (3).
2. Install the 3 water pump pulley bolts (1).
3. Install the drive belt. Refer to Drive Belt Replacement.

Caution: Refer to Fastener Caution in the Preface section.

4. Tighten the 3 water pump pulley bolts (1) to 20 N·m (15 lb ft)..

Note: Counterhold against crankshaft balancer bolt.

5. Install the air cleaner housing. Refer to Air Cleaner Assembly Replacement.