For 1990-2009 cars

#### Special Tools

CH-45004 Fuel Tank Drain Hose

For equivalent regional tools, refer to Special Tools.

Warning: Never drain or store fuel in an open container. Always use an approved fuel storage container in order to reduce the chance of fire or explosion.

Warning: Place a dry chemical (Class B) fire extinguisher nearby before performing any on-vehicle service procedures. Failure to follow these precautions may result in personal injury.

1. Remove the fuel fill cap.
2. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle.
3. Loosen the fuel fill pipe hose clamp at the fuel tank.
4. Separate the fuel fill pipe hose from the fuel tank.
5. Insert the CH-45004 drain hose into the fuel tank until the hose reaches the bottom of the fuel tank.
6. Use an hand or air operated pump device in order to drain as much fuel as possible.