For 1990-2009 cars

#### Special Tools

• | EN-48253 Accessory Belt Remover

• | EN-48952 Tensioner Spring Holding Pin

| For equivalent regional tools, refer to Special Tools.

1. Install the EN-48253 remover onto the tensioner and rotate the drive belt tensioner clockwise.
2. Rotate the drive belt tensioner (1) fully and simultaneously insert EN-48952 holder (2) to the drive belt tensioner pin hole.
3. Remove the generator and air conditioning compressor and power steering pump belt (4).