For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Disconnect battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove floor air outlet duct - left side. Refer to Floor Air Outlet Duct Replacement - Left Side.

1 | Air Inlet Valve Actuator Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

1. Disconnect electrical connector.
2. Remove air inlet valve actuator screws (Qty: 2)

Tip
For recalibration of the temperature valve actuator, refer to Actuator Recalibration.

Tighten
2.5 N·m (23 lb in)