For 1990-2009 cars

### Removal Procedure

1. Disconnect battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Disconnect the glow plug controller wiring harness plug (4).
3. Remove the glow plug controller bracket (2) from the battery tray.

### Installation Procedure

1. Install the glow plug controller bracket (2) at the battery tray.
2. Connect the glow plug controller wiring harness plug (4).
3. Connect battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.