For 1990-2009 cars

Application | Ref No. | Quantity | Size | Specification
--- | --- | --- | --- | ---
Metric | English
A/Trans Control Bolt | -- | -- | -- | 8 N·m | 71 lb in
A/Trans Flex Plate Bolt | -- | -- | -- | 60 N·m | 45 lb ft
A/Trans Fluid Pump Bolt to Converter Housing

- First Pass

200

8

M8x33

10 N·m

89 lb in

- Final Pass

200

8

M8x33

45°

A/Trans Fluid Pump Cover Bolt | 302 | 23 | M6x25 | 12 N·m | 106 lb in
Control Solenoid Valve Assembly (w/TCM and Body) to Case Bolt | 4 | 12 | M6x97 | 10 N·m | 89 lb in
Control Solenoid Valve Assembly (w/TCM and Body) to Case Bolt | 6 | 3 | M5x40.5 | 7 N·m | 62 lb in
Control Valve Body Assembly (Complete) Bolt | 400 | 1 | M5x40.5 | 7 N·m | 62 lb in
Control Valve Body to Case Bolt | 9 | 2 | M6x53 | 11 N·m | 97 lb in
Control Valve Body to Case Bolt | 10 | 9 | M6x60 | 11 N·m | 97 lb in
Control Valve Body Cover Bolt | 1 | 13 | M6x30 | 12 N·m | 106 lb in
Drain Plug | 64 | 1 | 1/8"-27 NPTF | 12 N·m | 106 lb in
Fluid Level Hole Plug | 63 | 1 | 1/8"-27 NPTF | 12 N·m | 106 lb in
Fluid Pressure Test Hole Plug | 51 | 1 | 1/8"-27 NPTF | 12 N·m | 106 lb in
Front Differential Carrier Baffle Bolt - Converter Housing | 204 | 2 | M6x25 | 12 N·m | 106 lb in
Front Differential Carrier Baffle Bolt - Case | 61 | 2 | M6x16 | 12 N·m | 106 lb in
Input Shaft Support Bolt | 57 | 3 | M6x50 | 12 N·m | 106 lb in
Input Speed Sensor Bolt | 21 | 1 | M6x23 | 12 N·m | 106 lb in
Manual Shift Detent Spring | 17 | 1 | M6x16 | 12 N·m | 106 lb in
Output Speed Sensor Bolt | 15 | 1 | M6x18 | 12 N·m | 106 lb in
Torque Converter and Differential Housing Bolt

- First Pass

27

15

M8x30

10 N·m

89 lb in

- Final Pass

27

15

M8x30

50°

--

Torque Converter to Flywheel Bolt | -- | -- | -- | 60 N·m | 45 lb ft
Transmission Bolt (1, 2, 3) - 6T40 | -- | -- | -- | 75 N·m | 56 lb ft
Transmission Bolt (4, 5) - 6T40 | -- | -- | -- | 50 N·m | 37 lb ft
Transmission Bolt (1, 2, 3, 4) - 6T45 | -- | -- | -- | 75 N·m | 56 lb ft
Transmission Bolt (5) - 6T45 | -- | -- | -- | 50 N·m | 37 lb ft
Transmission Bracket Mount to Mount Through Bolt | -- | -- | -- | 100 N·m | 74 lb ft
Transmission Fluid Cooler Outlet Pipe Nut | -- | -- | -- | 22 N·m | 17 lb ft
Transmission Fluid Cooler Pipe Inlet Nut | -- | -- | -- | 22 N·m | 17 lb ft
Transmission Mount Bolt | -- | -- | -- | 62 N·m | 46 lb ft
Transmission Mount Bolt - Left Side to Body | -- | -- | -- | 62 N·m | 46 lb ft
Transmission Mount Bolt - Left Side to Transmission | -- | -- | -- | 50 N·m + 60-75° | 37 lb ft
Transmission Mount Nut - Left Side to Body | -- | -- | -- | 62 N·m | 46 lb ft
Transmission Mount Through Bolt | -- | -- | -- | 62 N·m | 46 lb ft
Transmission Mount to Frame Bolt | -- | -- | -- | -- | --
Transmission Mount to Transmission Bolt | -- | -- | -- | 100 N·m | 74 lb ft
Transmission Range Selector Cable Bracket Bolt | -- | -- | -- | 18 N·m | 14 lb ft
Transmission Range Selector Lever Nut | -- | -- | -- | 20 N·m | 15 lb ft
*Reference number refers to the component callout number in Disassembled Views