For 1990-2009 cars

1. Install the catalytic converter clamp (1).
2. Install the catalytic converter (2).
3. Attach the catalytic converter clamp (1).

Caution: Refer to Fastener Caution in the Preface section.

4. Install the catalytic converter bracket bolt (3) and tighten to 40 N·m (30 lb ft) .
5. Tighten the catalytic converter clamp (1) to XXX N·m (XXX lb ft) .
6. Install the catalytic converter heat shield (2).
7. Install the 2 catalytic converter heat shield nuts (3) and tighten to 20 N·m (15 lb ft) .
8. Install the catalytic converter heat shield bolt (1) and tighten to 20 N·m (15 lb ft) .