For 1990-2009 cars

1. Install the 4 multiport fuel injector seals (6).
2. Install the multiport fuel injection fuel rail (4) and the fuel injectors (5) to the intake manifold (7).

Caution: Refer to Fastener Caution in the Preface section.

3. Install the 2 multiport fuel injection fuel rail bolts and tighten to 8 N·m (71 lb in).
4. Install the evaporative emission canister purge solenoid valve bracket (1) to the intake manifold (7).
5. Install the 2 evaporative emission canister purge solenoid valve bracket bolts (2) and tighten to 8 N·m (71 lb in).
6. Install the NEW intake manifold seal (3) to the intake manifold (2).
7. Install the NEW throttle body seal (1).
8. Install the intake manifold mount (2) to the intake manifold (1).
9. Install the manifold absolute pressure sensor (1) to the intake manifold (2).
10. Install the intake manifold absolute pressure sensor bolt and tighten to 6 N·m (54 lb in).