For 1990-2009 cars

### Diagnostic Instructions

• | Perform the Diagnostic System Check - Vehicle prior to using this diagnostic procedure.

• | Review Strategy Based Diagnosis for an overview of the diagnostic approach.

• | Diagnostic Procedure Instructions provides an overview of each diagnostic category.

### DTC Descriptor

DTC P0442 : Evaporative Emission (EVAP) System Small Leak Detected

### Circuit Description

This diagnostic tests the evaporative emission (EVAP) system for a small leak. The diagnostic runs when the ignition is in the OFF position, and the correct conditions are met. While the engine is operating, there are sources of heat transferred into the fuel tank from the following:

• | Exhaust heat

• | Engine heat

• | Ambient temperature

When the engine is stopped and the ignition is in the OFF position, a change in the fuel tank vapor temperature occurs. This results in a change in the pressure of the fuel tank vapor space. This change in pressure is monitored by the control module, using the fuel tank pressure (FTP) sensor input. The EVAP diagnostic detects leaks as small as 0.51 mm (0.02 in).

FTP Sensor Signal Voltage | Fuel Tank Pressure
--- | ---
High, Approximately 1.5 Volts or More | Negative Pressure/Vacuum
Low, Approximately 1.5 Volts or Less | Positive Pressure

### Conditions for Running the DTC

Note: The following conditions must be met prior to the ignition OFF test.

• | DTC P0100, P0101, P0102, P0103, P0111, P0112, P0113, P0116, P0117, P0118, P0119, P0128, P0443, P0446, P0449, P0450, P0451, P0452, P0453, P0455, P0458, P0459, P0496, P0497, P0498, P0499, P0560, P0562, P0563, P0700, P2227, P2228, or P2229 is not set.

• | The ignition voltage is greater than 11 volts.

• | A refueling event is not detected

• | The EVAP purge solenoid valve command is less than 26 percent.

• | The ambient air temperature (AAT) is between 2-32°C (35-90°F).

• | The engine coolant temperature (ECT) is less than 42°C (108°F) at start-up.

• | The ECT and the IAT are within 10°C (18°F) of each other at engine start-up.

• | The barometric pressure (BARO) is greater than 68 kPa.

• | The engine coolant temperature (ECT) during the previous ignition was greater than 74°C (165°F).

• | The fuel level is between 11-88 percent.

• | The vehicle traveled greater than 8 km (5 mi).

• | The engine run time is greater than 10 minutes.

• | DTC P0442 runs once per engine off cycle when the above conditions have been met prior to engine shut down.

### Conditions for Setting the DTC

The control module detects approximately 6 vacuum/pressure changes significantly less than a calibrated amount. The condition exists during the engine OFF test, then a 5 second delay for the MIL after engine start up.

### Action Taken When the DTC Sets

DTC P0442 is a Type A/B DTC.

### Conditions for Clearing the DTC

DTC P0442 is a Type A/B DTC.

### Diagnostic Aids

• | To improve the visibility of the smoke exiting the EVAP system, observe the suspected leak area from different angles with the J 41413-SPT High Intensity White Light.

• | To help locate intermittent leaks, use the J 41413-200 Evaporative Emissions System Tester (EEST) to introduce smoke into the EVAP system. Move all EVAP components while observing smoke with the J 41413-SPT . Introducing smoke in 15 second intervals will allow less pressure into the EVAP system. When the system is less pressurized, the smoke will sometimes escape in a more condensed manner.

• | Observe the Freeze Frame/Failure Records vehicle mileage since the diagnostic test last failed may help determine how often the condition occurs that caused the DTC to set. This may assist in diagnosing the condition.

### Reference Information

#### Schematic Reference

Evaporative Emissions Hose Routing Diagram

#### Connector End View Reference

Component Connector End Views

#### Description and Operation

Evaporative Emission Control System Description

#### DTC Type Reference

Powertrain Diagnostic Trouble Code (DTC) Type Definitions

#### Scan Tool Reference

Control Module References for scan tool information

#### Special Tools

• | J 41413-SPT High Intensity White Light

• | J 41413-VLV EVAP Port Vent Fitting Tool

• | J 41413-200 Evaporative Emissions System Tester (EEST)

• | J 41413-300 EVAP Cap and Plug Kit

• | CH-48096 EVAP Service Port Access Tool

• | GE-41415-50 Fuel Tank Cap Adapter

### Circuit/System Verification

1. Verify the following conditions do not exist in the EVAP system:

• | Loose, incorrect, missing, or damaged fuel fill cap

• | A damaged EVAP purge solenoid

• | Disconnected, incorrectly routed, kinked, or damaged EVAP pipes and hoses

• | A damaged EVAP vent valve or EVAP canister

⇒ | If you find any of the above conditions, repair as necessary.

Note: Refer to the J 41413-200 operation manual for detailed instructions.

2. Remove the fuel fill cap. Connect the GE-41415-50 to the fuel tank filler neck. Connect the J 41413-200 to the GE-41415-50 .
3. Calibrate the J 41413-200 Flow Meter to the correct leak orifice for the vehicle.
4. Command the EVAP vent solenoid closed with a scan tool.

Note: Larger volume fuel tanks and/or those with lower fuel levels may require several minutes for the floating indicator to stabilize.

5. Activate the J 41413-200 and compare the flow meter's stable floating indicator position to the red flag. The floating indicator should be below the red flag.

⇒ | If the floating indicator is above the red flag, test for a leak in the EVAP system.

6. Operate the vehicle within the Conditions for Running the DTC to verify the DTC does not reset. You may also operate the vehicle within the conditions that you observed from the Freeze Frame/Failure Records data.

### Circuit/System Testing

Note:

• | You must start with the Circuit/System Verification before proceeding with Circuit/System Testing.

• | Ensure that the vehicle underbody temperature is similar to the ambient temperature and allow the surrounding air to stabilize before starting the diagnostic procedure. The system flow will be less with higher temperatures.

1. Connect the GE-41415-50 to the fuel tank filler neck. Connect the J 41413-200 to the GE-41415-50 .
2. Connect the CH-48096 between the EVAP purge solenoid and the EVAP purge pipe.
3. Turn the nitrogen/smoke valve on the control panel to SMOKE.
4. Command the EVAP vent solenoid closed with a scan tool.
5. Use the remote switch to introduce smoke into the EVAP system.
6. Use the J 41413-VLV to open the EVAP service port. Once smoke is observed, remove the J 41413-VLV .

Note: Introduce smoke at 15 second intervals while testing the system.

7. Verify that smoke is not exiting the entire EVAP system with the J 41413-SPT .

Note: The fuel tank may need to be lowered to improve visibility of some of the EVAP system components.

⇒ | If smoke is observed, repair the condition as necessary.

8. Remove the J 41413-200 nitrogen supply hose from the GE-41415-50 , and remove the GE-41415-50 from the fuller neck.
9. Install the fuel fill cap.
10. Connect the J 41413-200 nitrogen/smoke supply hose to the EVAP service port of the CH-48096 .
11. Command the EVAP vent solenoid closed with a scan tool.
12. Use the remote switch to introduce smoke into the EVAP system.

Note: The fuel tank may need to be lowered to improve visibility of some of the EVAP system components.

13. Verify that smoke is not exiting the entire EVAP system with the J 41413-SPT .

⇒ | If smoke is observed, repair the condition as necessary.

14. Verify the individual EVAP system components for a leak using the J 41413-300 . The EVAP system components should not leak.

⇒ | If a condition is found replace the affected component.

### Repair Instructions

• | Fuel Tank Pressure Sensor Replacement

• | Evaporative Emission Canister Purge Solenoid Valve Replacement

• | Evaporative Emission Canister Vent Solenoid Valve Replacement

• | Evaporative Emission Hoses/Pipes Replacement - Chassis/Canister

• | Evaporative Emission Canister Replacement

### Repair Verification

1. Turn the nitrogen/smoke valve to nitrogen.
2. Command the EVAP vent valve closed with a scan tool.
3. Use the remote switch to activate the J 41413-200 .
4. Use the remote switch to introduce nitrogen and fill the EVAP system until the floating indicator stabilizes.
5. Verify the flow meter's stable floating indicator position is at or below the red flag.
6. Remove the CH-48096 , and connect the purge line to the EVAP purge solenoid.
7. Clear the DTCs with a scan tool.