For 1990-2009 cars

### Removal Procedure

1. Remove the luggage carrier. Refer to Luggage Carrier Replacement.

Warning: Refer to Safety Glasses Warning in the Preface section.

2. Drill through the luggage carrier rivnut head using a 7.5 mm (0.295 in) drill bit.
3. Remove the rivnut from the roof.

### Installation Procedure

1. Using a 10 mm (0.3937 in) drill bit, drill the rivnut hex shape hole in the roof out to a round 10 mm hole.
2. Install a replacement rivnut to the hole in roof using a rivnut tool, or equivalent.
3. Install the luggage carrier. Refer to Luggage Carrier Replacement.