For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. If equipped with FWD, remove the intermediate drive shaft. Refer to Front Wheel Drive Intermediate Shaft Replacement.
2. Support the engine. Refer to Engine Support Fixture.
3. Remove the exhaust flexible pipe. Refer to Exhaust Flexible Pipe Replacement.

1 | Rear Engine Mount Upper Nut Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

1. Remove and discard engine mount nut.
2. Apply threadlocker to the engine mount threads. Refer to Adhesives, Fluids, Lubricants, and Sealers.

Tip

• | The engine mount nuts must be replaced once removed. Allow adhesive on new engine mounts nuts to cure for 24 hours after replacement.

• | Use engine support fixture to raise engine.

Tighten
50 N·m (37 lb ft)

2 | Rear Engine Mount Bracket Bolt Tighten 58 N·m (43 lb ft)
3 | Rear Engine Mount Bracket Bolt Tighten 22 N·m (16 lb ft)