For 1990-2009 cars

## Instrument Panel Compartment Door Dampener Replacement Acadia

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the instrument panel compartment trim plate. Refer to Instrument Panel Compartment Trim Plate Replacement .

1 | Instrument Panel Compartment Dampener Assembly

#### Procedure

Twist the dampener and pull outward to remove from the dampener from the instrument panel assembly.

## Instrument Panel Compartment Door Dampener Replacement Enclave

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the instrument panel compartment door stops and open door fully.

1 | Instrument Panel Compartment Dampener Assembly

#### Procedure

Twist the dampener and pull outward to remove from the dampener from the instrument panel assembly.

## Instrument Panel Compartment Door Dampener Replacement OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the instrument panel compartment trim plate. Refer to Instrument Panel Compartment Trim Plate Replacement.

1 | Instrument Panel Compartment Dampener Assembly

#### Procedure

Twist the dampener and pull outward to remove from the dampener from the instrument panel assembly.

## Instrument Panel Compartment Door Dampener Replacement Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the instrument panel compartment door stops and open door fully.

1 | Instrument Panel Compartment Dampener Assembly

#### Procedure

Twist the dampener and pull outward to remove from the dampener from the instrument panel assembly.