For 1990-2009 cars

## Rear Side Door Garnish Molding Replacement Enclave

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear side door trim panel. Refer to Rear Side Door Trim Panel Replacement.

1 | Rear Side Door Upper Garnish Molding Retainer (Qty: 2) Tip Use a door trim panel removal tool or equivalent to aid in the removal of the retainer.
2 | Rear Side Door Upper Garnish Molding Tip Pull outward starting at the front and moving slowly rearward to remove the molding.