For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the right and left catalytic converters. Refer to Catalytic Converter Replacement - Left Side and Catalytic Converter Replacement - Right Side .
3. Support the transaxle with a transaxle jack.

1 | Rear Transaxle Brace Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 50 N·m (37 lb ft)
2 | Rear Transaxle Brace Bolt Tighten 50 N·m (37 lb ft)
3 | Rear Transaxle Brace