For 1990-2009 cars

## Side Marker Lamp Bulb Replacement OUTLOOK HID

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement .
2. Remove the headlamp assembly. Refer to Headlamp Replacement .

1 | Front Side Marker Lamp Bulb

#### Procedure

Rotate the lamp socket and remove the bulb.

## Side Marker Lamp Bulb Replacement OUTLOOK Non HID

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement .
2. Remove the headlamp assembly. Refer to Headlamp Replacement .

1 | Front Side Marker Lamp Bulb Tip Rotate the lamp socket and remove the bulb.