For 1990-2009 cars

## Parking and Front Fog Lamp Bracket Replacement Enclave

### Removal Procedure

1. Remove the front wheelhouse liner. Refer to Front Wheelhouse Front Liner Replacement.
2. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement.
3. Remove the lower front bumper fascia to bracket screw (1).
4. Remove the 3 upper and 3 lower screws (2).
5. Remove the lower push lock retainer (4) and bolt (3).
6. Release the two fog lamp bracket tabs from the front bumper fascia, push in order to release the tabs.
7. Remove the parking and front fog lamp bracket (1) from the front bumper fascia (2).

### Installation Procedure

1. Position and align the parking and front fog lamp bracket (1) to inside the front bumper fascia (2).
2. Secure the locking tabs to the front bumper fascia.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the lower push lock retainer (4) and bolt (3).
4. Install the 3 upper and 3 lower screws (2).
5. Install the front bumper lower fascia to bracket screw (1) and tighten to 2.5 N·m (22 lb in).
6. Install the front bumper fascia. Refer to Front Bumper Fascia Replacement.
7. Install the front wheelhouse liner. Refer to Front Wheelhouse Front Liner Replacement.