For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front seat back cushion cover j-clips and reposition the seat back cushion cover to gain access to the lumbar support and bolts.

1 | Front Seat Lumbar Assembly Bolt (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
2 | Front Seat Lumbar Assembly

#### Procedure

Disconnect the electrical connector.