For 1990-2009 cars

## Radiator Grille Support Reinforcement Replacement Acadia, Enclave

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement.
2. Remove the front bumper center filler. Refer to Front Bumper Center Filler Replacement.
3. Remove the front bumper molding. Refer to Front Bumper Fascia Molding Replacement.

1 | Front Fascia Reinforcement Screw (Qty: 6) Caution: Refer to Fastener Caution in the Preface section. Tighten 7 N·m (62 lb in)
2 | Front Fascia Reinforcement