For 1990-2009 cars

## Windshield Washer Hose Replacement Acadia

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the hood insulator. Refer to Hood Insulator Replacement .

1 | Windshield Washer Nozzle

#### Procedure

1. Disconnect the washer hose.
2. Pinch the washer nozzle tabs and push outward from the hood to remove.

2 | Windshield Washer Nozzle Hose Assembly Elbow
3 | Windshield Washer Nozzle Hose Assembly Tee
4 | Windshield Washer Nozzle Hose Assembly

#### Procedure

1. Disconnect the integral clip from the driver side hood hinge in order to release the hose from the hinge.
2. Disconnect the washer hose from the washer pump hose connection.

## Windshield Washer Hose Replacement Enclave

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the hood insulator. Refer to Hood Insulator Replacement .

1 | Windshield Washer Nozzle

#### Procedure

Disconnect the washer hose from the washer nozzles.

2 | Windshield Washer Hose Assembly
3 | Windshield Washer Hose Hood Hinge Clip

#### Procedure

1. Disconnect the integral clip from the driver side hood hinge in order to release the hose from the hinge.
2. Disconnect the washer hose from the washer pump hose connection.

## Windshield Washer Hose Replacement OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the hood insulator. Refer to Hood Insulator Replacement .

1 | Windshield Washer Nozzle

#### Procedure

1. Disconnect the washer hose.
2. Pinch the washer nozzle tabs and push outward from the hood to remove.

2 | Windshield Washer Nozzle Hose Assembly Elbow
3 | Windshield Washer Nozzle Hose Assembly Tee
4 | Windshield Washer Nozzle Hose Assembly

#### Procedure

1. Disconnect the integral clip from the driver side hood hinge in order to release the hose from the hinge.
2. Disconnect the washer hose from the washer pump hose connection.